**Open Wobble Switch: QC Guide**

|  |  |
| --- | --- |
|  | Solder on the correct PCB side All component will be **inserted** on the PCB side that says “Top” and **soldered** on the side marked “Bottom”. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |